MagnaCheck

Tangential Field Strength Meter

	
	3D Probe
	1D Probe

	Measurement range
	To 2000 Gauss
	To 1000 Gauss

	Units
	Gauss, mTesla, Ka/m

	Measurement modes 
	DC, AC peak, true RMS

	MPI bench support 
	True RMS for thyristor switched fields
	True RMS and shot time measurement**

	Peak hold mode 
	Off, 1, 2, 5 and 10 seconds

	Measurement sample rate 
	70 samples/second
	500 samples/second

	Measurement resolution
	0.16 Gauss
	0.1 Gauss

	Probe types 
	3D Auto Recognition
	1D Transverse

	Sensor calibration
	Stored digitally in probe

	Measurement accuracy 
	1%

	Standards compliance
	ASTM E1444/1444M-12 and EN ISO 9934-3

	Zeroing
	Manual zero with null pot supplied

	Display type
	Colour LCD with selectable backlight

	Display size and resolution 
	2.8”  / 70mm - 320x240 pixels

	Power
	2 x 1.5V AA batteries

	Typical battery life
	In excess of 10 hrs continuous use

	Instrument dimensions 
	6.5x3.2x1 inch  /  163x80x25mm 

	Instrument weight
	0.77 lb  / 350g including batteries


** Available in 1D mode as option

. 
